VEHICLE DETAILS - 2000 CHEVROLET 1500 4X2 EXT SILVERADO

VIN: 1GCEC19T4YZ333843 Body Style: XCAB Top Type: Hard Top

Ext Color: RED Int Color: BLK Odometer: 153,428

 Grade 2.9 Below Average

 More About Auto Grade

 MSRP-Not Available

 Engine Starts-Yes

 Drivable-Yes

\*Process protected under U.S. Patent No. 8,320,362

 VALUE ADDED OPTIONS

 CD Player

 VEHICLE INFORMATION

OPTIONS

 50 State Emissions

 A/C

 Auxiliary Pwr Outlet

 Cloth Seats

 Dual Air Bags

 Front Floor Mats

 Front Reading Lamps

 Maintenance Book

 Owner's Manual

 Power Mirrors

 Power Windows

 Pwr Steering

 Side Air Bags

 Tire Pressure Monitor System

 Traction Control

 Trip Counter

 Two-Wheel Drive

 US EPA Label

 Warranty Books

MECHANICAL

 8 Cylinder Gas

 Automatic Transmission

 Pwr Brakes

 5.3 L

INTERIOR

 Odometer - 6 Digits Digital -Operable

 Int Odor: OK

 Cloth

 Regular Dash

TIRES AND WHEELS

Wheels: Wheels

Tire Tread Depth Brand Size

Left Front: 4/32" GOODYEAR 275/45R20

Left Rear: 7/32" GOODYEAR 275/45R20

Right Front: 6/32" GOODYEAR 275/45R20

Right Rear: 6/32" GOODYEAR 275/45R20

KEYS

 Master Key - 1

ADDITIONAL INFORMATION

 AS IS,

Common Abbreviations

Minor Damages Conventional Repairs May Be Required-[2 Items]

IMAGE DESCRIPTION CONDITION SEVERITY

L Cab Side L Cab Side Dent/Paint Dmg 1" to 2"

RF Door Dent/Paint Dmg 3" to 4"

Paint and Body Requires Conventional Repair-[3 Items]

IMAGE DESCRIPTION CONDITION SEVERITY

F Metal Bumper Chrome F Metal Bumper Chrome Dent/No Paint Dmg 3" to 4"

LF Fender LF Fender Dent/Paint Dmg 4" to 5"

R Bed Side R Bed Side Scratch Heavy 4" to 5"

Miscellaneous-[5 Items]

IMAGE DESCRIPTION CONDITION SEVERITY

Front Emblem Broken Replacement Required

Mechanical-[2 Items]

IMAGE DESCRIPTION CONDITION SEVERITY

Radiator Leak Repair Required

Water Pump Leak Repair Required

VIN: 1GCEC19T4YZ333843